**REQ.NO.:05**

|  |  |  |  |
| --- | --- | --- | --- |
| **QTY** | **UNIT** | **DESCRIPTION** | **ITEM** |
| **500 000** | **Metre** | **PIPES 42"**  **\*Pipe line carbon steel seamless or ASW welded (1 weld) beveled end according to ANSI B16.25,length of 9to12 metres,supplied with protective end caps**  **\*Size 42 INCH out side diameter X0.500"(12.7mm) WT. X APL 5Lgrade (X 60)**  **\*Each pipe shall be externally coated with extruded polyethylene coating with 3mm (As Aminimum) asper din 30670 with standing temp.80C min.** | **01** |
| **52000** | **NOS** | **\*Heat shrinkable sleeves suitable for item(01) open type width should be suitable with bar distance of ends for item(01) plus 2"**  **\*Explry period for heat shrine kable sleeves not less than (5) years arrival basrah**  **\*pipe coating of open type storeg at (0-60)C** | **02** |
| **140** | **NOS** | **\*Equipment and tools required for work above item (02)** | **03** |
|  |  | **The supplier shall be under take the following**  **1- The value of Bid bond is 7000.000$ to be submitted with the offer.**  **2- Relevant catalogues, diagrams and data sheets (Chemical composition,Dimension,Weights,mechanical and Hydrostatic test) to be submitted with the offer**  **3- Numbering and marking for each pipe by Heating stamp, including the necessary data such as pipe length,Diameter,Thickness,Grade**  **4- Third party inspection required**  **Country of manufacturer origin :-**  **ITALY , FRANCE , JAPAN , USA , UK,OCRANIA ,INDIA** |  |